MOD.030118

|  |
| --- |
| ANAGRAFICA DEL PRODUTTORE |
| DENOMINAZIONE SOCIALE |  |
| Codice fiscale /Partita Iva: |  |
| Sede Legale: |  |
| Sede Operativa: |  |
| IMPIANTO DI PRODUZIONE |
| Indirizzo |  |
| Autorizzazione /data rilascio/Ente rilasciante |  |
| Descrizione e caratteristiche del processo di produzione |  |
| AUTORIZZAZIONE IN BASE ALLA QUALE E’ STATO GENERATO EOW |
| Tipologia, numero e data di rilascio AIA / AUA/Com. |  |
| Quantitativo EOW generabile da Autorizzazione (oppure limite autorizzato In ingresso a trattamento)  |  |
| CERTIFICAZIONE (n. data di scadenza) |  |
| DESCRIZIONE EOW |
| CATEGORIA MERCEOLOGICA (Norma Ceca/Eurofer) |  |
| Certificato di controllo radiometrico D.Lgs 152/2006 (Reg. UE 333/2011) |  |
| Presenza assenza Allegato III Reg. 333/2011 /UE |  |
| Il produttore dichiara che:* Il rottame è generato ai sensi dell’art. 184 ter D.lgs. 152/06.
* Il rottame EOW generato non contiene più del 2% in peso di materiale estraneo (sterili).
* Il rottame non contengono ossido di ferro in eccesso, salvo quantità dovute allo stoccaggio all’aperto in condizioni atmosferiche normali di rottami preparati.
* Il rottame EOW NON presenta le esclusioni di cui al punto 2 Allegato 1 al Regolamento 31-03-2011 n. 333/2011/UE (sostanze pericolose comprese oli e grassi, limatura, scaglie e polveri contenenti fluidi quali oli o emulsioni oleose, fusti e contenitori che contengono o hanno contenuto oli e vernici).
* Il rottame EOW non contiene materiale radioattivo.
* Il rottame EOW NON presenta alcune delle caratteristiche di pericolo di cui al punto 1.6 Allegato 1 al Regolamento 31-03-2011 n. 333/2011/UE.
* Il rottame EOW non contiene alcun contenitore sotto pressione chiuso o insufficientemente aperto che possa causare esplosioni in forno.
* Il rottame EOW Non è sottoposto a Normativa ADR per il trasporto.
* Il rottame EOW conferito è conforme a quanto indicato nella presente scheda descrittiva e a quanto riportato dall’allegato III al Reg. 333/2011/UE e quanto indicato è veritiero e reale e si assume ogni responsabilità civile o penale nel caso di dichiarazione infedele.
* Eventuali variazioni a quanto dichiarato verranno comunicate tempestivamente.

NOTE: ……………………………………………………………………………………………………………………………………………………………………………………. |

Data:………………………………….

 FIRMA DEL LEGALE RAPPRESENTANTE

 ………………………………………………………………………………………..

MOD.030118

|  |
| --- |
| PRODUCER’S DETAILS |
| COMPANY NAME |  |
| Tax code/ VAT code: |  |
| Head office: |  |
| Operating site: |  |
| PRODUCTION PLANT |
| Address |  |
| Authorization /date of issue /Issuing body |  |
| Description and characteristics of the production process |  |
| AUTHORIZATION ON THE BASIS OF WHICH EOW WAS GENERATED |
| Type, number and date of issue of AIA / AUA/Com. |  |
| Volume of EOW that can be generated by Authorization ( aut. In input)  |  |
| CERTIFICATION (expiration date and number) |  |
| EOW DESCRIPTION |
| PRODUCT CATEGORY (ECSC/Eurofer rules) |  |
| Radiometric control certificate Legis. Decree 152/2006 (Reg. UE 333/2011) |  |
| Presence absence Annex III Reg. 333/2011 /UE |  |
| The producer declares that:* The scrap is generated as per art. 184 ter Legis. Decree 152/06.
* The EOW scrap generated does not contain more than 2% in weight of extraneous (sterile) material.
* The scrap does not contain excess ferrous oxide, except for amounts due to storage in the open air in normal conditions for prepared scrap.
* The EOW scrap does NOT present the exclusions as per point 2 Annex 1 to the Regulations of 31-03-2011 no. 333/2011/UE (hazardous substances including oils and grease, filings, scale and dust containing fluids such as oils or oily emulsions, drums or containers which contain or have contained oils and paint).
* The EOW scrap does not contain radioactive material.
* The EOW scrap does NOT present any of the hazard characteristics as per point 1.6 Annex 1 of Regulations of 31-03-2011 no. 333/2011/UE.
* The EOW scrap does not contain any closed or insufficiently open pressure vessels which may cause explosions in the furnace.
* The EOW scrap is not subject to ADR transport regulations.
* The EOW scrap delivered complies with the indications of the present descriptive file and to what is shown in Annex III to rule 333/2011/UE and what is indicated is true and real and it assumes all civil and penal responsibility in the case of untrue declaration.
* Any variations to the declarations shall be communicated promptly.

NOTE: ……………………………………………………………………………………………………………………………………………………………………………………. |

Date:………………………………….

 SIGNATURE LEGAL REPRESENTATIVE

 ………………………………………………………………………………………..